|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1 | A |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Workstation 2 sends a packet to workstation 3. Workstation 2 sends a packet to workstation 5. Workstation 1 sends a packet to workstation 2. Workstation 2 sends a packet to workstation 3. Workstation 2 sends a packet to workstation 6. Workstation 6 sends a packet to workstation 3. Workstation 5 sends a packet to workstation 4. Workstation 2 sends a packet to workstation 1. Workstation 1 sends a packet to workstation 3. Workstation 1 sends a packet to workstation 5. Workstation 5 sends a packet to workstation 4. Workstation 4 sends a packet to workstation 5

Port A Port B

2 6

1 5

4

2. Class B

3.

Network mask

255.255.255.192

6 bit for subnet mask

2^6 = 64

177.56.42.63

4. 192.168.11.0/24

254 subnet

Server ip 192.168.1.1

Rest up to 192.169.1.101

2^6

5.

Dynamic NAT IP change